**PuTTY Presets for UHF and Kenwood**

**Common Errors:**

* Make sure that the COM port that you are connecting to correct by checking the drivers.
* Make sure UHF and Kenwood loaded preset are COM11 and COM4 respectively

**UHF:**

Serial line: COM11

Speed: 9600

Connection type: Serial

Data bits: 8

Stop bits: 1

Parity: None

Flow control: XON/XOFF

Local echo: Forced on

Local line editing: Forced off

**Kenwood:**

Serial line: COM4

Speed: 9600

Connection type: Serial

Data bits: 8

Stop bits: 1

Parity: None

Flow Control: XON/XOFF

Local echo: Forced on

Local line editing: Forced off